Figure Propellant and oxidizer pouring/draining valves arrangement and pipe diameter (8-1-1)

Figure 2FT design for propellant and oxidizer mixing in payload propulsion subsystem (8-3-1)